Below are the details of the raw data for the paper: High density optical storage using plasmonic color nano pixels as dual-state data-bits.

Files:

Closeup SEM showing typical 250x250 period array of blue-yellow pixels (120x220nm arm lengths [designed]) in Figure 1.TIF
Used in Figure 1 as a typical example of the most densely packed arrays, with the largest difference between the length of each arm. 

Original image of color palette used in Figure 1, x-axis polarised.jpg
Original image of color palette used in Figure 1, y-axis polarised.jpg
Original camera images taken from the switchable color palette shown in Figure 1.

Raw spectrometer data files for spectra found in Figure 1
Original transmission data that was used to generate the graphs seen in Figure 1 and Figure S1.

Original image used in Figure2, x-axis polarised
Original image used in Figure2, y-axis polarised
Original camera images taken from the switchable image arrays shown in Figure 2.

Original QR image used in Figure 3, x-axis polarised
Original QR image used in Figure 3, y-axis polarised
Original camera images taken from the switchable QR code shown in Figure 3.

SEM of upper left corner of the QR code shown in Figure 3
Original SEM image used to show the pixel arrangement that forms the upper left hand corner of the QR code shown in Figure 3.